NETWORK CONFIGURATION
=====================

OpenVPN consists of two sides of network configuration.  One side is the
*link* between the local and remote side, the other side is the *virtual
network adapter* (tun/tap device).

.. include:: link-options.rst
.. include:: vpn-network-options.rst
.. include:: virtual-routing-and-forwarding.rst
